**POV INSPECTION CHECKLIST**

POV Inspection Checklist Page 1 of 2

**NAME**

**SECTION**

**Veh Make / Model**

**/**

**Drvr Lic #/ Exp Date**

**/**

**Veh Color / Year**

**/**

**Lic Plate # / Exp Date**

**/**

**ITEM WHAT TO CHECK WHAT TO LOOK FOR CHECKOFF**

**TIRES** Condition Tread depth, wear, weathering, evenly seated, Front Rear

bulges, imbedded objects, cuts, breaks. At least

NOTE: No mixing of radial on mm of tread over entire surface tires/bias tires. (Use a penny and place it in the tire tread

(Lincoln’s head facing you and toward the tire).

If you can see all of Lincoln’s head it is not ok)

Spare tire Spare tire (inflated), jack, lug wrench Pass Fail

**LIGHTS** Head lights Both high and low beams operational, cracked, Left Right condensation, secured

Tail lights Lenses intact, tail lights work when turned on Left Right (red)

Brake lights Lenses intact, brake lights work when brake is Left Right applied (red)

Turn signals Lenses intact, left and right turn signals blink Front Left Front (red lights in rear and yellow lights in front) Right

Rear

Left Rear

Right

Backup lights Lenses intact, left and right backup lights work Left Right

(White Light)

Four-way flashers Lenses intact, left and right turn signals Front Left Front

flash/blink at the same time Right

Rear

Left Rear

Right

License plate light Lenses in tact, does light stay on Pass Fail

**Windshield** Windshield Not cracked, broken or scratched to the degree Pass Fail

**/ Windows /** that impairs vision

**Wipers** Rear Window Not cracked, broken or scratched to the degree Pass Fail

that impairs vision

Windows Windows go up and down, not scratched or tinted Pass Fail to the degree that impairs vision

Window Controls Check handles, push electric buttons Pass Fail

Windshield Wipers Both wipers are installed on vehicle, windshield Pass Fail wipers work, blades show signs of wear

**Mirror** Mirror outside Missing, cracked Pass Fail

Mirror inside Missing, cracked Pass Fail

**Bumpers** Bumper Front Missing, lose, broken Pass Fail Bumper Rear Missing, lose, broken, bent in any way Pass Fail

to cause a hazard

**POV INSPECTION CHECKLIST – cont.**

Inspector’s Name

 Signature

Operator’s Name

Platoon Sergeant/ NCOIC Approval

Date Inspection Conducted

Leave / Pass / Holiday Dates

 Signature

 Signature

Date of Follow-up

 Inspection if necessary

POV Inspection Checklist Page 2 of 2

**Brakes** Brakes Foot pedal cannot travel more than half way to Pass Fail floor, does brake light stay on

Emergency Brake Properly adjusted, check emergency brake by: Pass Fail

pull/push emergency brake, apply foot brake, gently press gas pedal and ensure brake holds vehicle

**Interior** Horn Does it work Pass Fail Defroster front Ensure hot air blows out above the dash Pass Fail Defroster Rear Check light on dash, if in the winter, ensure it Pass Fail

works by allowing the rear windshield to clear up

Emergency equipment (OPTIONAL) First aid kit, warning triangle, Pass Fail flashlight, fire extinguisher, blanket, flares,

shovel, chains, tools, etc. (Check host nation laws for any additional equipment required)

Heater Ensure heater works Pass Fail

**Seatbelts** Seatbelt Front/Rear Missing, frayed, does not snap Front Rear (Include shoulder harness

during inspection, may have a center seat belt)

**License /** State drivers license Expired, missing Pass Fail

**Decals /** Installation Decal Missing, needs replacing Pass Fail

**Insurance** License Plate (License plates Expired, check sticker/decal to ensure plate is Pass Fail match windshield decal – current

Europe only)

Insurance Does the operator have valid insurance Pass Fail

**Under the** Brake Filled to the appropriate level Pass Fail

**Hood** Windshield washer Windshield washer fluid (increased usage during Pass Fail

winter months)

Battery Check the color indicator on the battery – check Pass Fail terminals, clean and tight, battery held down

securely

Power steering Filled to appropriate level Pass Fail Hoses Cuts, cracks, leaks, bulges, chaffing, Pass Fail

deterioration